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	Sr. No.
	Specifications (Existing)
	Specifications (Amended)
	Quantity 

	3
	UV/Vis Dual Beam Spectrophotometer:                                               Wavelength range:   190—1100 nm
Spectral bandwidth:  Fix 1.4 nm
	Wavelength range:   190—900 nm
Spectral bandwidth:  < 1.5 nm
	3

	4
	FTIR Spectrometer (Bench-Top):                                                                 Spectral range: 6,000 to 500 cm-1 with Zn Se beamsplitter
Interferometer:                             RockSolid , permanent aligned, High stability
Detector:                                        DigiTect detector system, high sensitivity room temperature,                                           
Spectroscopy software:       OPUS or equivalent: easy-to-use, full GLP compliant,
Integrated Platinum-ATR-accessory, Diamond, 1 bounce, QuickLock
Specifications:
- Diamond crystal, single reflection, edged in tungsten carbide
- Work disk: stainless steel
- Spectral range: 10-8,000cm-1
- Ergonomic one-finger clamp mechanism
- Pressure control
- Working distance (max. sample height) >20mm
- Easy cleaning due to the rotatable pressure applicator
- Exchangeable crystal plates (Diamond, Ge)
- Purgeable and sealed beam path
- Sample compartment cover adapted for Platinum-ATR-accessory.                    
	Spectral range: 6,000 – 500 cm-1 with Zinc Selenide Optics
Interferometer:                     permanently aligned, High stability                                          Detector:                              Highly sensitive, room temperature
Spectroscopy software:       Included, Easy-to-use, Complete package
ATR-accessory, Diamond
	1

	9
	Glass Distillation Unit, Complete with Mountable Accessories:                  Output: 20 ltr/hr 
	Output: 4 Ltr/hr or above
	3

	10
	Electronic/Analytical Balance (Four Digit):                                        Digital, Capacity upto 250 grams Readability:  0.001 mg, Linearity: ±0.002 mg, Calibration: External
	10A
	Analytical Balance:                                                                                          Capacity: 220 grams or above, Readability:  0.001 g, Linearity: ±0.002 g, Calibration: Internal/External
	6

	
	
	10B
	Analytical Balance:                                                                                          Capacity: 220 grams or above, Readability:  0.0001 g, Linearity: ±0.0002 g, Calibration: Internal/External
	4
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