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GOVT COLLEGE UNIVERSITY FAISALABAD


TENDER NOTICE No. 209

                            Sealed Tenders are invited from the firms / suppliers of repute, which are registered with Sales Tax and Income Tax Departments and must be original manufacturer or their authorized dealers only for the supply, installation and establishment of FM Radio Station for the Department of Mass Communication, GC University Faisalabad, to be delivered/installed/set up at University Campus at the designated place on turnkey basis. Details of equipment and its quantity with complete specifications is available in the Tender Documents. Tender documents can be obtained from the office of the undersigned from 07 – 10 – 2013 during working hours on payment of Rs. 1000/- (Rs. One Thousand only). The tender must be submitted before 24 – 10 – 2013  and will be opened at 1400 hours on the same day by the Tender opening/Purchase Committee in the presence of Vendors/ Firms or their representatives who wish to attend. Call Deposit in the form of a CDR/Bank Draft in favour of Treasurer, GC University, Faisalabad, valuing equal to 2% of the Bid Cost must be attached with the bid, no bid will be entertained without call deposit of 2 % of the quoted value. Tender documents can also be downloaded from GCUF website (www.gcuf.edu.pk) and/or PPRA website (www.ppra.org.pk) and, in this case, tender fee (Rs. 1000.00) will be attached with bid proposal in the form of a CDR / Bank Draft in the name of Treasurer, GCUF.




Convener
FM Radio Station Purchase Committee
GC University Faisalabad
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TENDER NOTICE No.209


INVITATION OF TENDER FOR THE SUPPLY,  INSTALLATION AND ESTABLISHMENT OF FM RADIO STATION  FOR DEPARTMENT OF MASS COMMUNICATION, GC UNIVERSITY FAISALABAD

Purchase Price: Rs. 1000/-

Sealed Tenders are invited from the firms / Suppliers of repute which are registered with Sales Tax and Income Tax Departments and must be OEM or their authorized Dealers/ sole distributors, for the supply, installation and establishment of FM Radio Station for Department of Mass Communication, GC University Faisalabad, as per Appendix “A”.To be delivered at University Campus on turnkey basis and must include 5 years for Transmitter &three years’  for Antenna system parts replacement warrantee from the principle. . Bidding is to be single stage – two envelope procedure as per PPRA rule no. 36 (b).


GENERAL TERMS & CONDITIONS

1. Tender Opening Date:

The tender must reach the office of the undersigned on or before 
24 October 2013 at 1200 Hours which will be opened on same day 
at 1400 Hours in the office of the Convener Tender opening/Purchase Committee in the presence of the firms or their  authorized representatives who wish to attend.
The bid will be opened for technical evaluation only as single stage two envelop procedure would be adopted and 70:30  shall be the evaluation criteria.
2. Bid Security and Performance Security:

· A Call Deposit Receipt at the rate of 2% of the tendered amount (refundable) (Cheque not acceptable) in the name of the Treasurer, GC University, Faisalabad must be attached with the tender without which the tender may be rejected by the authority concerned.
· The rates / bids should be inclusive of all applicable Govt. Taxes.
· 10 % of the total bill shall be retained by the university as performance warrantee and shall be returned after expiry of the warrantee period.


3. Validity of Offers.

· Offers shall be valid for at least 180 days from the date of submission of bids.
· Withdrawal / modification of the original offer within the validity period shall entitle the University to forfeit earnest   money.
· The Competent Authority reserves the right to increase or decrease quantities.  


4. Failures and Terminations: 

	No offer of a supplier / firm will be considered if:-
a) Received without Earnest Money / Call Deposit or less CDR than the required.
b) Bidder shall submit bid according bid documents of GCUF, alternate bids will not be considered.  							
c) Received later than the date and time fixed for tender.
d) The tender is incomplete in any respect or is unsigned. 
e) The offer is ambiguous and the offer is conditional.
f)         The offer from a firm which is black listed at any level.
g)      Any erasing cutting / overwriting etc. will not be accepted.
h) The supplier fails to deliver the consignment within the specified   delivery  period strictly in accordance with the terms and conditions as laid down in 	the Purchase Order; 
i) The University is authorized to forfeit the earnest money if desired and the firm may also be black listed.



5. Other special condition
        
a. The party has to sign MOU/agreement attached as appendix B with GCUF.
b. After receipt/Installation/Establishment of FM Radio station the inspection will be carried out by the end user department within one week.
c. The whole project is to be awarded to one company on turnkey basis i.e. the same company shall carry out all the work services and provide 5 years on Transmitter, 3 years on antenna system & one year on site warrantee with all the spare support what so ever. 
d. The decision of the Vice Chancellor of GC University, Faisalabad, would be final & binding on both the parties and not challengeable in any court of law.


e. The GCUF reserve the right to reject any or all of the tenders without
assigning any reason thereof.
f. Catalogue / literature of the equipment/material supplied must be enclosed with the equipment / material.
g. All Government Taxes will be deducted according to applicable rules. 
h. The bidder only to be authorized partner / sole distributor of the original manufacturer in Pakistan, if not then bid may be rejected. 
i. The bidders may not propose any kind of refurbished hardware / Radio equipment / component in their bid.
j.  Letter of authorization / sole distributorship Certificate from principal / Manufacturer must be attached with the Customer list also must be attached.
k. Minimum 50 FM Radio Stations or more has to be installed by bidder in all over Pakistan, if not then bid will be rejected.   
l. No alternate or optional offer/ bid will be considered. 
m. All equipment must be made in USA/ Japan/ Europe.

ISSUED TO

M/S--------------------------------------------------------------------------------------------------
-------------------------------------------------------------------------------------------------------


Convener
 FM Radio Station 
   Purchase Committee


















									Appendix “A”
									To Tender No. 209


TENDER NOTICE No. 209

DETAILED SPECIFICATIONS AND REQUIREMENTS TO ESTABLISH FM RADIO STATION

	1
	TRANSMITTER AND ANTENNA SYSTEM
	 Qty

	
	Transmitter


	Complete solid state 1 KW FM Transmitter with Built in Stereo Generator card,  Freq. Range  87.5-108MHZ. P.S & Exciter separate, internal cooling , SMS to pre feeded mobile nos. in case of fault ,Modular system, 150 W Exciter, Temp. Range, up to 50
	1

	
	 
	 Deg centigrade. C , Power supply -190 to 280 watts 50 Hz,Rack for transmitter, warranty 5 years comprehensive onsite with parts and labor warranty from principle   (Orgin USA, JAPAN, Europe)
	

	
	
	
	

	
	Antenna
	 4-Bays Dipole antennas Hot dip galvanized steel average gain 1.8dBd (8dBd) VSWR< 1.1, Connector 7/16 N female , Band With 87.5-108 MHz Almost circular radiation pattern, with RF power splitter and Harness Cables
	 

	
	 
	 with Helix low loss 80 Meter cable , 100 % imported & no local parts to be quoted or supplied .  3 year warranty 
	 

	
	Tower
	Guy Supported Triangular 18 inch pipe gage 14,  150 feet height, Hot dipped galvanized , red oxide and professionally  painted (red & White) wires 6mm, anti-turn arrangement, tower light with sun switch (imported), cable tray upto transmitter room, light eraster, high quality installation, every wire clamped, cable tray with 14 gage sheet and 3 year warranty from principle.
	1

	
	Tower Earthing
	Grounding less than 1 ohm , 6 mm Copper wire lightening Arrestor and copper Rod.
	 

	
	Installation Of Tower
	Installation of tower with grounding less the 1 ohm
	1

	
	 
	
	

	 
	ON  Air Studio
	 

	4
	ON  Air Studio
	
	

	
	
	Digital /Analouge  On-Air Console,14 to 16 channel, 6 mic channel  and 4 line channel, telephone hybrid line input.
	1

	
	
	Telephone Hybrid           
	1

	
	
	ON Air Light
	2

	
	
	Head Phone Amplifier
	1

	
	
	
	

	
	
	Audio Tuner
	1

	
	
	Temperature alarm for Transmitter ( message to predefined mobile nos.)
	

	
	
	Head Phones
	5

	
	
	 Telephone Device for live out door broadcast filip Jack Type
	1

	
	
	Vocal Microphone with Pop up  Filter
	4

	
	
	Phantom Power Mic Microphone with Pop up  Filter
	2

	
	
	Mic Stand with boom  (imported)
	2

	
	
	Mic Table Stand            (Imported)
	4

	
	
	 2 channel , Small mixer for out door 
	1 

	
	
	4 Channel ,Handy Mp-3 professional recorder with built in 5 capsules
	1 

	
	
	Monitor Speakers 
	1 Pair

	
	
	
	

	
	
	
	

	 
	Production Studio
	 

	5
	Production Studio + On air Studio Back up
	
	1

	
	
	Digital / Manual On-Air Console,16 channels, 6 Mic channel 4 line channel and telephone hybrid system input
	1

	
	
	Telephone Hybrid                    
	1

	
	
	ON Air Light
	1

	
	
	Head Phone Amplifier
	1

	
	
	Professional CD/DVD player
	1

	
	
	Tuner
	1

	
	
	Head Phones
	4

	
	
	Cardioid Dynamic Microphone with pop up  filter 
	1

	
	
	Vocal Microphone with pop up  filter
	3

	
	
	Mic Stand with boom
	1

	
	
	Mic Table Stand
	3

	
	
	Monitor Speakers
	1 Pair

	
	
	 2 channel , Small mixer for out door
	01

	
	
	4 Channel ,handy Mp-3 professional recorder with built in 5 capsules
	01 

	 
	 
	
	

	6
	Power 
	 

	
	
	
	

	
	
	
	 

	
	Isolation Transformer
	Isolation Transformer 10 KVA
	1

	
	AVR
	Automatic Voltage Regulator 10  KVA
	1

	
	UPS
	 UPS ( 7KVA for Transmitter and 2 KVA for Equipment) Purely Sine Wave having Minmum 30 Minutes back up time
	1

	
	
	
	1

	
	EARTHING
	Earthing of Transmission & PIE rack & Generator
	1

	 
	 
	
	 





Connectors & Audio Cables:

S. No.  Description/Specifications                   			   Qty
	1
	AudioCableDoubleCorewithshield(Length:200Mtr)
	4

	2.
	XLRConnector
	100

	3.
	Phonopinconnector
	75

	43
	TR Satudio jack
	30


	

Sound proofing & Development of Transmitter Room :

S. No.  Description/Specifications                   			Qty
	1
	Sound proofing of ON AIR Studio with wood panneling  and masonite sheets
	1

	2.
	Sound proofing of OFF AIR Studio with wood panneling  and masonite sheets
	           1

	3.
	Transmitter Room designed for Transmitter 
	1




Details of Call Deposit/DD/CDR                                                Signature____________________

No_______________Amount___________                             Name of Bidder_______________

Bank______ Branch_____ City__________                              CNIC No ___________________

Name of the Firm & Address _____________________________________Ph No____________

	
Convener
FM Radio Station 
Purchase Committee 
GC University Faisalabad
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