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	  TENDER NOTICE NO. 212 / 2014



            Government College University, Faisalabad (GCUF) invites sealed tenders / bids from the well reputed firms / importers / suppliers, registered with Sales Tax and Income Tax Departments, for procurement of following (04) Lab Equipments for Department of Food Science. Detail and Specifications are attached in the Tender Documents.

	S.No
	Name of Equipment
	Description

	A.
	High Performance Liquid Chromatography (HPLC)
	Pump, Gradient Unit, Auto sampler, Diode Array Detector, Organizer,  Column Oven, Accessories

	B.
	Twin-Screw Extruder
	Mod. PEX 1 N Complete Capacity 1 Liter with Double Chamber, Accessories

	C.
	Sonication Apparatus

	Mod. PEX 1 N complete capacity 1 liter with double chamber, Accessories

	D.
	Elisa Micro Plate Reader
	Elisa Plate Reader, Accuracy at 450.492nm, Precision/Reproducibility at 450.492nm, Linearity



1. Tender Documents are available for download at GCUF's website www.gcuf.edu.pk and PPRA's website  www.ppra.punjab.gov.pk.  The procurement shall be completed in accordance with Punjab Procurement Rules 2014, on Single Stage - Two Envelope Bidding Procedure.
2. A single package containing two envelopes, Technical and Financial separate Bids, duly completed, signed, stamped, sealed and in complete conformity with Tender Documents should be dropped in Tender Box placed at Procurement Department of the GCUF, not later than 1200 Hrs on 15.05 2014 . Technical Bids will be opened first on 15.05.2014 at 1230 Hrs, and Financial Bids will be opened (as per schedule issued later on) for only those Successful Technical Bids which are acceptable to the "Technical Committee". Whereas, Financial Bids of unsuccessful Bidders will be returned un-opened..
3. All bids must be accompanied by Tender Fee Rs; 4,000/- and Bid Security (Refundable) at the rate of 2% of total Tender/Bid value in shape of CDRs in favor of "Treasurer GCUF". The CDRs of Tender Fee and Bid Security (in original) must be attached with Technical Bid & Financial Bid, respectively. Bids which are incomplete, not signed,  not stamped,  not sealed, without tender fee & bid security, late or submitted by other than specified mode will not be considered.
4. Income/Sales Tax Registration Certificate, CNIC and other documents as mentioned in the Tender Documents must accompany the bids. Taxes will be deducted as per GOP rules.
5. GCUF Management may reject  any or all bids at any time prior to the acceptance of a bid, as provided under Rule-35 of Punjab Procurement Rules, 2014.
 
(Dr. Iftikhar Hussain Bukhari)
Advisor Procurement and Inventory Control 
Allama Iqbal Road Faisalabad, Phone: 041-9201032
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	TENDER DOCUMENTS NO. 212 / 2014



SUPPLY OF LAB EQUIPMENTS
FOR DEPARTMENT OF FOOD SCIENCE.
                                                                                                                         Purchase Price: Rs. 4000/-
									   @Rs: 1000/- per Equipment

Sealed Tenders are invited from the firms / Suppliers of repute which are registered with Sales Tax and Income Tax Departments for the supply of (4) Lab Equipments like High Performance Liquid Chromatography (HPLC), Twin-Screw Extruder, Sonication Apparatus, Elisa Micro Plate Reader & other related items for the Department of Food Science. Detail and Specifications are separately attached as Appendix “A”.

GENERAL TERMS & CONDITIONS

1. Tender Opening Date & Procedure: 

· The procurement shall be completed in accordance with Punjab Procurement Rules 2014, on Single Stage - Two Envelope Bidding Procedure.
· A single package containing two envelopes, Technical and Financial separate Bids in complete conformity with Tender Documents will be dropped in Tender Box placed at Procurement Department of the GCUF, not later than 1200 Hrs on 15.05 2014 . 
· Technical Bids will be opened first on 15.05.2014 at 1230 Hrs. for evaluation by the " GCUF Technical Committee".  
· Financial Bids of Successful Technical Bidders will be opened as per schedule issued later on. 
· Financial Bids of unsuccessful Bidders will be returned un-opened.

2. Tender Fee, Bid Security and Performance Security:

· Technical Bid must be accompanied by Tender Fee of Rs:4,000/- @ Rs:1,000/- per equipment in shape of Call Deposit Receipt (CDR) in original. 
· Financial Bid must be accompanied by Bid Security @ 2% of the tendered bid / value (refundable) in shape of Call Deposit Receipt (CDR) in original.
· CDRs must be in favor of Treasurer, GC University, Faisalabad.
· The rates / bids should be inclusive of all applicable Govt. Taxes.
· Performance warrantee  @10 % of the total bill shall be retained by the university and refundable after expiry of the warrantee period.

3. Validity of Offers.

· Offers shall be valid for at least 180 days from the date of submission of bids.

· Withdrawal / modification of the original offer within the validity period shall entitle the University to forfeit Bid Security.
· The Competent Authority reserves the right to increase or decrease quantities.


4. Failures and Terminations: 

	No offer of a supplier / firm will be considered if:-

a) Bid received without Bid Security / Call Deposit or less CDR than the required.
b) Bids received not in accordance with specifications of Tender Documents.
c) Alternate bids  received or alternative equipment offered.  	
d) Bid received later than the date and time fixed for tender.
e) Tender is incomplete in any respect or is unsigned.
f) Offer is ambiguous and the offer is conditional.
g) Offer from a firm which is black listed at any level.
h) Any erasing / cutting / overwriting etc. 
i) The supplier fails to deliver the consignment within specified delivery period strictly in accordance with the terms and conditions as laid down in the Purchase Order. 
j) Situation warranted, then University is authorized to forfeit the bid Security and the firm may also be black listed.

5. Other special condition
        
a) Bids should contain complete detail / brochure from manufacturing companies and definite information of accessories, country of origin, warranty period, after sale spare parts & service etc about quoted items.
b) Successful bidder will be bound to provide manual, warranty document and   technical support or training of quoted equipment, wherever applicable.
c) After receipt of the items the inspection will be carried out by the end user department within 15 days.
d) The decision of the Vice Chancellor of GC University, Faisalabad, would be final & binding on both the parties and not challengeable in any court of law.
e) The quantities can be increased / decreased by the Competent Authority.
f) The performance security applicable under the rules shall be deducted from the final bill of the successful bidder.
g)  All Government Taxes will be deducted according to applicable rules.
h) The GCUF reserve the right to reject  any or all bids at any time prior to the acceptance of a bid, as provided under Rule-35 of Punjab Procurement Rules, 2014.

ISSUED TO


M/S--------------------------------------------------------------------------------------------------
-------------------------------------------------------------------------------------------------------
                                                                                 
          


                                                                                             Dr. Iftikhar Hussain Bukhari
                                                                                    Advisor, Procurement & Inventory Control  
                                                            


									                           Appendix “A”		
	TENDER NOTICE NO. 212 / 2014



DETAIL & SPECIFICATIONS OF LAB EQUIPMENTS
FOR DEPARTMENT OF FOOD SCIENCE.

	Sr. No.
	Item Name
	Specifications
	Quantity Required
	Cost(PKR)

	High Performance Liquid Chromatography (HPLC)     (USA, Europe, Japan)

	1. 
	Pump
	Liquid Feed System: Dual plunger reciprocating pump (series connection, pulsation suppression)
Flow rate rang: 0.001 to 9.999 ml/min
Maximum Discharge Pressure: 39.2 MPa (0.001 to 5.000 mL / min) & 19.6 MPa (5.001 to 9.999 mL / min)
Flow Rate Accuracy: +2 L / min) +2% (0.101 to 8.0 mL / min) & + 4 % (8.001 to 9.999 mL / min)
Flow Rate Stability: SD 0.02min or RSD 0.075 %, Whichever is larger (retention time at 1.0 mL / min)
Degasser: 6-Channel 
	1
	

	2.
	Gradient Unit
	LiqNumber of solutions mixable: 4 solutions
Mixing system: Solenoid valve opening/closing time control system
Recommended flow rate range: 0.4 to 1.8 mL/min.
	1
	

	3.
	Autosampler
	Number of standard samples 1.5 mL x 200 pcs,
Sample injection system: Direct injection system
Syringe capacity (standard): 100 μL
Sample injection volume: 0.1 to 50 μL (standard syringe),
Injection volume reproducibility: 0.3 % RSD (when 10 μL is injected) 

	1
	

	

4.
	

Diode Array Detector
	

Number of photodiode bits		1024
Light source				D2 lamp, W lamp, Hg lamp (for wavelength check)
Wavelength range 190 to 900 nm
Wavelength accuracy + 1 nm
Noise	0.5 x 10-5 AU or less (250 / 600 nm)
Drift	0.5 x 10-3 AU/hr or less (250 / 600 nm)
Spectrum acquisition cycle Selectable from 50, 100, 200, 400, 800, 1600, 3200 msec
	1
	

	5.
	Organizer
	Power supply	 AC 100 to 240 V (50/60 Hz), 350VA
Output DC 24V, 300W (provides DC power supply for 1110 pump x1, 1210 Autosampler x 1, 1410UV / 1430DAD x1)
Space to accommodate solvent bottles 314(W) mm x 280.8(D) mm
	1
	

	6.
	Column Oven
	Temperature control system Block heating + Air circulation system
Temperature setting range	1 to 65C (in 1C step)
Temperature control range (ambient temperature – 15C) to (ambient temperature + 50C)
Temperature control accuracy + 0.1C
Column accommodated Up to 3 columns (250mm length max.)
	1
	

	7.
	Accessories
	Pump seal washing kit
Complete unit with software and computer
	1
	

	Twin-Screw Extruder

	1.
	Mod. PEX 1 N Complete Capacity 1 Liter with Double Chamber,
	- Allows to work from tub of 0.2 to 1 liter
- Durable tub, stir rod, all in stainless steel.
- Double chamber for quicker water cooling. Chiller not supplied
- Quick connecting attachments for optional cooling/heating.
- Stainless steel container for module control.
- Tubular cables with quick connecting attachments.
- Ultrasound control timer 0-30 min.
- Variable speed mixer with rods and stainless steel attachments.
- Operating manual
- Power 200W 230V 50-60 Hz
-Dimensions of generator 250x 150 x 360, of stative 250x330xh780mm
- Weight without stirring rod Kg.35
	1
	

	2.
	Accessories
	Appliance Cryotherm CP 02
- Heating/cooling group to control circuitry with double chamber or serpentine of the extractors as previously described.
- 6 liter tub with circulation pump
- From +100 °C to – 25 °C with digital control
- Usage of 200W to – 20°C, 150W to 0 °C, 2000 W for other temperatures.
- Complete with attachments and accessories
- Dimensions 235 x 445 x 620 mm 
- Weight 34 Kg
	1
	

	Sonication Apparatus

	1.
	Mod. PEX 1 N complete capacity 1 liter with double chamber
	- Allows to work from tub of 0.2 to 1 liter
- Durable tub, stir rod, all in stainless steel.
- Double chamber for quicker water cooling. Chiller not supplied
- Quick connecting attachments for optional cooling/heating.
- Stainless steel container for module control.
- Tubular cables with quick connecting attachments.
- Ultrasound control timer 0-30 min.
- Variable speed mixer with rods and stainless steel attachments.
- Operating manual
- Power 200W 230V 50-60 Hz
- Dimensions of generator 250x150x360, of stative 250x330xh780mm
- Weight without stirring rod Kg.35
	1
	

	2.
	Accessories
	Appliance Cryotherm CP 02
- Heating/cooling group to control circuitry with double chamber or serpentine of the extractors as previously described.
- 6 liter tub with circulation pump
- From +100 °C to – 25 °C with digital control
- Usage of 200W to – 20°C, 150W to 0 °C, 2000 W for other temperatures.
- Complete with attachments and accessories
- Dimensions 235 x 445 x 620 mm 
- Weight 34 Kg

	1
	

	Elisa Micro Plate Reader  (USA, UK, Germany, Japan)

	1.
	Elisa Plate Reader, 
	Light Source: 	LED, Self Calibration
Detectors: Silicon photodiode
Measurement channel: 8+1 reference
Wavelength range: 400-750nm
Wavelength selection: Filter (8 filter position)
Supplied filters: 405, 450, 492 and 620nm
Plate formats:	 96well (including strip microplate)
Measurement range:	 0-4 OD
Resolution: 0.0001 OD
	1
	

	2.
	Accuracy at 450.492nm
	0.000 - 2.000 OD: < (0.5% + 0.10 OD) typical
2.000 – 3.000 OD: < (1.0% + 0.010 OD) typical
	1
	

	3.
	Precision/Reproducibility at 450.492nm
	0.000 - 2.000 OD: < (0.5% + 0.005 OD) typical
2.000 – 3.000 OD: < (1.0% + 0.005 OD) typical
	1
	

	4.
	Linearity
	0.000 - 2.000 OD: < 1%
2.000 – 3.000 OD: < 1.5%
Computer interface:	USB 1.1/2.0
Shaking: Linear with 4 modes
Power supply:	 100-240AC, 50/60Hz auto sensing
%	0.0 to 199.9%; 200 to 400%
Measurement Range	: mg/L 	0.00 to 19.99; 20.0 to 45.0 mg/L
Ppm    0.00 to 19.99; 20.0 to 45.0 ppm
Temp. 	0 to 50 °C
%   	0.1%; 1%
Measurement Resolution: 
mg/L    	0.01 mg/L; 0.1 mg/L
ppm 		0.01 ppm; 0.1 ppm
Temp. 		0.1 °C
mmHg  	375 to 825 mmHg
Barometric range: 	
mbar 		500 to 1100 mbar
hPa 		500 to 1100 hPa
mmHg  	1 mmHg

Barometric resolution 	
Mbar 		1 mbar
hPa 		1 hPa
Accuracy: 	± 1%; ± 0.3 °C
Salinity compensation;  0.0 to 50.0 ppt
Calibration: 	1 or 2 points
Memory 	30 sets, last calibration       
                        data
Display 	liquid crystal
IP rating 	IP54
Input 		BNC; Cinch (NTC    
                       30  kΩ)
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Details of Call Deposit Receipt (CDR)                              Signature_____________________

No:_______________Amount:___________                           Name of Bidder_______________

Bank______ Branch_____ City__________                          CNIC No ______________________

Name of the Firm & Address _____________________________________Ph No____________

	
                                                                                             
                                                                                         Dr. Iftikhar Hussain Bukhari
                                                                 Advisor, Procurement & Inventory Control                                                                                            
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